**2,000 Mile Inspection**

# Mechanic’s Name: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Bus # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Mileage: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\*\*Special Notice\*\* In the event the mechanic is not familiar with the correct clearances, adjustments, specifications, or encounters any other mechanical defect not shown in the following instructions, it will be the mechanic’s responsibility to obtain proper instruction from manufacturer.

Symbol Definition: \_\_\_\_\_O.K. \_\_\_\_\_Adjusted \_\_\_\_\_Repair Needed

Lubrication: Heating & Air Conditioning:

\_\_\_\_\_Engine Oil \_\_\_\_\_Check Heater Cores for Leaks

\_\_\_\_\_Automatic Transmission Fluid Level \_\_\_\_\_Check Op. of Evap. & Blower Motors

\_\_\_\_\_Check Rear Axle Oil Level \_\_\_\_\_Check Op. of Under Seat Blow Motors

\_\_\_\_\_Complete Chassis Lubrication \_\_\_\_\_Check Op. of Htr. Modulation Valve

\_\_\_\_\_Check Power Steer Fluid Level \_\_\_\_\_Check Op. of Booster Pump

\_\_\_\_\_Check All Oil Lines & Connections \_\_\_\_\_Clean Condenser Coil & Replace

Evaporator Filter Screens

Cooling System: \_\_\_\_\_Clean Air Intake Filter Screens

\_\_\_\_\_Check Coolant Level \_\_\_\_\_Check Air Cond. Compressor Oil Level

\_\_\_\_\_Check Antifreeze @ \_\_\_\_\_\_\_\_

\_\_\_\_\_Check All Connections & Fittings

Suspension & Steering: Windshield Wipers:

\_\_\_\_\_Check Steering Linkage & Lubricate \_\_\_\_\_Check Wiper Operation

\_\_\_\_\_Check Power Steering Hose & Lines \_\_\_\_\_Check Washer Operation

\_\_\_\_\_Visual Wheels Tires & Check Pressure \_\_\_\_\_Lub All Wiper Linkage

\_\_\_\_\_Tighten Wheel Nuts/Clock Wheels-Centered

\_\_\_\_\_Check Tire Wear for Alignment

\_\_\_\_\_Check Air Springs for Cracks, Abrasions , Interior:

or Other Damage \_\_\_\_\_Check Drivers Seat Adjustment & Lube

\_\_\_\_\_Check All Mirrors

Fuel System: \_\_\_\_\_Check Emergency Exits & Alarms

\_\_\_\_\_Check Fuel Cap Gasket \_\_\_\_\_Check Fire Extinguisher

\_\_\_\_\_Check Exhaust System \_\_\_\_\_Check First Aid Kit/Contents

\_\_\_\_\_Examine All Connections \_\_\_\_\_Check Seats for Vandalism

\_\_\_\_\_Check All Grab Rails for Tightness

Brakes: \_\_\_\_\_Check Rear Door –Exit/Alarm/Seal

\_\_\_\_\_Drain Air Tanks

\_\_\_\_\_Check & Tighten Air Lines and Connections Wheelchair Lift:

\_\_\_\_\_Check Brake Lining (5/15 or less, realign) \_\_\_\_\_Check Wheelchair Lift Operation

\_\_\_\_\_Check All Fittings/Leaks & Damage

Electrical: \_\_\_\_\_Check Roller Track Panel V-Groove

\_\_\_\_\_Check Headlights,Clearance,Turn Signals Rollers for Allignment

\_\_\_\_\_Check Interior Lights \_\_\_\_\_Check Platform Panel Hinge for

\_\_\_\_\_Check Horn Operation Alignment,Binding or Wear

\_\_\_\_\_Check Wheelchair Restraints for

Proper Operation